,Model##OTHER##,Desired Door Width##LENGTH##INCHES,Desired Door Height##LENGTH##INCHES,Product Page URL##OTHER##
BA-FRI-SS-8-8,BA-FRI-SS-8-8,8,8,https://www.bestaccessdoors.com/8-x-8-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-10-10,BA-FRI-SS-10-10,10,10,https://www.bestaccessdoors.com/10-x-10-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-12-12,BA-FRI-SS-12-12,12,12,https://www.bestaccessdoors.com/12-x-12-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-14-14,BA-FRI-SS-14-14,14,14,https://www.bestaccessdoors.com/14-x-14-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-16-16,BA-FRI-SS-16-16,16,16,https://www.bestaccessdoors.com/16-x-16-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-18-18,BA-FRI-SS-18-18,18,18,https://www.bestaccessdoors.com/18-x-18-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-22-22,BA-FRI-SS-22-22,22,22,https://www.bestaccessdoors.com/22-x-22-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-22-30,BA-FRI-SS-22-30,22,30,https://www.bestaccessdoors.com/22-x-30-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-22-36,BA-FRI-SS-22-36,22,36,https://www.bestaccessdoors.com/22-x-36-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-24-24,BA-FRI-SS-24-24,24,24,https://www.bestaccessdoors.com/24-x-24-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-24-36,BA-FRI-SS-24-36,24,36,https://www.bestaccessdoors.com/24-x-36-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-24-48,BA-FRI-SS-24-48,24,48,https://www.bestaccessdoors.com/24-x-48-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-30-30,BA-FRI-SS-30-30,30,30,https://www.bestaccessdoors.com/30-x-30-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-32-32,BA-FRI-SS-32-32,32,32,https://www.bestaccessdoors.com/32-x-32-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-36-36,BA-FRI-SS-36-36,36,36,https://www.bestaccessdoors.com/36-x-36-fire-rated-insulated-access-panel-in-stainless-steel/
BA-FRI-SS-48-48,BA-FRI-SS-48-48,48,48,https://www.bestaccessdoors.com/48-x-48-fire-rated-insulated-access-panel-in-stainless-steel/
"CUSTOM SIZE (Width Min 8""- Max 48"" | Height (Min 8""- Max 48"" )",CUSTOM,24,24,https://www.bestaccessdoors.com/48-x-48-fire-rated-insulated-access-panel-in-stainless-steel/
