,Model##OTHER##,Desired Door Width##LENGTH##INCHES,Desired Door Height##LENGTH##INCHES,Product Page URL##OTHER##
BA-FRN-DF-8-8,BA-FRN-DF-8-8,8,8,https://www.bestaccessdoors.com/8-x-8-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-10-10,BA-FRN-DF-10-10,10,10,https://www.bestaccessdoors.com/10-x-10-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-12-12,BA-FRN-DF-12-12,12,12,https://www.bestaccessdoors.com/12-x-12-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-14-14,BA-FRN-DF-14-14,14,14,https://www.bestaccessdoors.com/14-x-14-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-16-16,BA-FRN-DF-16-16,16,16,https://www.bestaccessdoors.com/16-x-16-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-18-18,BA-FRN-DF-18-18,18,18,https://www.bestaccessdoors.com/18-x-18-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-22-22,BA-FRN-DF-22-22,22,22,https://www.bestaccessdoors.com/22-x-22-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-22-30,BA-FRN-DF-22-30,22,30,https://www.bestaccessdoors.com/22-x-30-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-22-36,BA-FRN-DF-22-36,22,36,https://www.bestaccessdoors.com/22-x-36-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-24-24,BA-FRN-DF-24-24,24,24,https://www.bestaccessdoors.com/24-x-24-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-24-36,BA-FRN-DF-24-36,24,36,https://www.bestaccessdoors.com/24-x-36-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-30-30,BA-FRN-DF-30-30,30,30,https://www.bestaccessdoors.com/30-x-30-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-32-32,BA-FRN-DF-32-32,32,32,https://www.bestaccessdoors.com/32-x-32-fire-rated-access-panel-non-insulated-with-mud-in-flange/
BA-FRN-DF-36-36,BA-FRN-DF-36-36,36,36,https://www.bestaccessdoors.com/36-x-36-fire-rated-access-panel-non-insulated-with-mud-in-flange/
"CUSTOM SIZE (Width Min 8""- Max 36"" | Height (Min 8""- Max 36"" )",CUSTOM,36,36,https://www.bestaccessdoors.com/36-x-36-fire-rated-access-panel-non-insulated-with-mud-in-flange/

