,Model##OTHER##,Door Width##LENGTH##INCHES,Door Height##LENGTH##INCHES,Product Page URL##other##
BA-UAP-PF-8-8,BA-UAP-PF-8-8,8,8,https://www.bestaccessdoors.com/8-x-8-universal-access-panel-with-plaster-flange/
BA-UAP-PF-10-10,BA-UAP-PF-10-10,10,10,https://www.bestaccessdoors.com/10-x-10-universal-access-panel-with-plaster-flange/
BA-UAP-PF-12-12,BA-UAP-PF-12-12,12,12,https://www.bestaccessdoors.com/12-x-12-universal-access-panel-with-plaster-flange/
BA-UAP-PF-14-14,BA-UAP-PF-14-14,14,14,https://www.bestaccessdoors.com/14-x-14-universal-access-panel-with-plaster-flange/
BA-UAP-PF-16-16,BA-UAP-PF-16-16,16,16,https://www.bestaccessdoors.com/16-x-16-universal-access-panel-with-plaster-flange/
BA-UAP-PF-18-18,BA-UAP-PF-18-18,18,18,https://www.bestaccessdoors.com/18-x-18-universal-access-panel-with-plaster-flange/
BA-UAP-PF-22-22,BA-UAP-PF-22-22,22,22,https://www.bestaccessdoors.com/22-x-22-universal-access-panel-with-plaster-flange/
BA-UAP-PF-24-24,BA-UAP-PF-24-24,24,24,https://www.bestaccessdoors.com/24-x-24-universal-access-panel-with-plaster-flange/
"CUSTOM SIZE (Width Min 8""- Max 24"" | Height (Min 8""- Max 24"" )",CUSTOM,24,24,24-x-36-universal-access-panel-with-plaster-flange/